{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Tableau des pressions saturante","Hygrométrie"],"not_rendered":{"charts":1,"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tableau des pressions saturante","index":0,"n_rows":46,"n_cols":3,"rows_kept":46,"flags":["formulas_cached_only"]}
["Températures (°C)","Masse d'eau par kg d'air sec (g/kg)","Pression saturante (Pa)"]
[-20,0.63,103]
[-19,0.7,113]
[-18,0.77,125]
[-17,0.85,137]
[-16,0.93,151]
[-15,1.01,165]
[-14,1.11,182]
[-13,1.22,199]
[-12,1.34,218]
[-11,1.46,238]
[-10,1.6,260]
[-9,1.75,284]
[-8,1.91,310]
[-7,2.08,338]
[-6,2.27,368]
[-5,2.47,402]
[-4,2.69,438]
[-3,2.94,476]
[-2,3.19,518]
[-1,3.47,563]
[0,3.78,611]
[1,4.07,658]
[2,4.37,706]
[3,4.7,759]
[4,5.03,814]
[5,5.4,873]
[6,5.79,935]
[7,6.21,1002]
[8,6.65,1074]
[9,7.13,1149]
[10,7.63,1229]
[11,8.15,1313]
[12,8.75,1404]
[13,9.35,1498]
[14,9.97,1600]
[15,10.6,1706]
[16,11.4,1819]
[17,12.1,1939]
[18,12.9,2066]
[19,13.8,2199]
[20,14.7,2339]
[21,15.6,2488]
[22,16.6,2646]
[23,17.7,2811]
[24,18.8,2986]

{"sheet":"Hygrométrie","index":1,"n_rows":25,"n_cols":4,"rows_kept":25,"merged":[[9,0,9,2],[10,0,10,2],[11,0,11,2],[12,0,12,2],[13,0,13,2]],"flags":["formulas_cached_only"]}
["1. Calculer Rth [m²°C/W] et φ [W /m²] du mur."]
["Désignation ","Épaisseur (en m)","λ","R "]
["Rsi"]
[{"$nulls":3},""]
[{"$nulls":3},""]
[{"$nulls":3},""]
[{"$nulls":3},""]
[{"$nulls":3},""]
["Rse"]
["Résistance thermique R (m²°K/W)",null,null,{"v":0,"d":"0.000"}]
["Coefficient de transmission U (W/m²°K)",null,null,{"$error":"#DIV/0!"}]
["Ti"]
["Te"]
["Φ",null,null,{"$error":"#DIV/0!"}]
[]
["2. Tracer le diagramme des températures."]
[null,"Épaisseur","Température"]
["Ti =",-0.1,{"v":0,"d":"0.00"},"°C"]
["tsi =",0,{"$error":"#DIV/0!"},"°C"]
["t1 =",0,{"$error":"#DIV/0!"},"°C"]
["t2 =",0,{"$error":"#DIV/0!"},"°C"]
["t3 =",0,{"$error":"#DIV/0!"},"°C"]
["t4 =",0,{"$error":"#DIV/0!"},"°C"]
["tse =",0,{"$error":"#DIV/0!"},"°C"]
["te =",0.1,{"$error":"#DIV/0!"},"°C"]